[bookmark: _GoBack][image: ]
image1.emf
TANK TYPESHAZARDS

285  Ballast Stab Cofferdam

285.003  Rig Chain Tanks

285.005  Roll 

Reduction Tanks

285.006  Heeling 

Tanks

285.007  

Cofferdams

Lack of oxygen

x x

Presence of inert gases

x x

H2S

x

CO

x

CHx

circulation of air limited (single 

manhole entry)

x x

distance from clean air inlet

Other

Poor visibility

x

Working at height harness needed

Manholes on floor Fall from height

Tripping hazard (bulks /beams / pipes)

Low heights head injury (bulks /beams 

/ pipes)

x

Uneven deck

x

Rust leading to sharp edges

slippery deck

x

Toxic Vapors

Flammable vapors / explosion

x x

Pathogenic (ie. Sewage)

Pressure built in

presence of electrical cables

Pipes under pressure

x

several manholes to pass horizontally

x

several manholes to pass vertically

volume Confined space not 

appropriate for SCBA

Tripod not adapted to location 

(Height/width)

x x

Rescue kit not adapted to location 

(horizontal rescue)

STRING Lack of oxygen

Presence of inert gases

CO

circulation of air limited (single manhole entry)

Uneven deck



Lack of oxygen

Presence of inert 

gases

H2S



circulation of air 

limited (single 

manhole entry)

Poor visibility

slippery deck

Flammable vapors / 

explosion

Tripod not adapted to 

location 

(Height/width)



Low heights head 

injury (bulks /beams 

/ pipes)

Flammable vapors / 

explosion

Pipes under pressure

several manholes to 

pass horizontally

Tripod not adapted to 

location 

(Height/width)



General 

hazards

Tank content 

related 

hazards

Impairment of 

rescue related 

hazards

TANK TYPES

HAZARDS

Gaseous 

Hazards


